Static Call Graph - [STM32F3_blinkingLEDs\STM32F3_blinkingLEDs.axf]

# Static Call Graph for image STM32F3_blinkingLEDs\STM32F3_blinkingLEDs.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Fri Mar 15 17:54:02 2019

### Maximum Stack Usage = 136 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - ADC3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - ADC4_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - BusFault_Handler from stm32f3xx_it.o(i.BusFault_Handler) referenced from startup_stm32f303xc.o(RESET)
  - CAN_RX1_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - CAN_SCE_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - COMP1_2_3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - COMP4_5_6_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - COMP7_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - DebugMon_Handler from stm32f3xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f303xc.o(RESET)
  - EXTI0_IRQHandler from stm32f3xx_it.o(i.EXTI0_IRQHandler) referenced from startup_stm32f303xc.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - EXTI2_TSC_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - FLASH_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - FPU_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - HardFault_Handler from stm32f3xx_it.o(i.HardFault_Handler) referenced from startup_stm32f303xc.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - MemManage_Handler from stm32f3xx_it.o(i.MemManage_Handler) referenced from startup_stm32f303xc.o(RESET)
  - NMI_Handler from stm32f3xx_it.o(i.NMI_Handler) referenced from startup_stm32f303xc.o(RESET)
  - PVD_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - PendSV_Handler from stm32f3xx_it.o(i.PendSV_Handler) referenced from startup_stm32f303xc.o(RESET)
  - RCC_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - Reset_Handler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - SPI1_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - SPI2_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - SPI3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - SVC_Handler from stm32f3xx_it.o(i.SVC_Handler) referenced from startup_stm32f303xc.o(RESET)
  - SysTick_Handler from stm32f3xx_it.o(i.SysTick_Handler) referenced from startup_stm32f303xc.o(RESET)
  - SystemInit from system_stm32f3xx.o(i.SystemInit) referenced from startup_stm32f303xc.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM1_BRK_TIM15_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM1_TRG_COM_TIM17_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM1_UP_TIM16_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM2_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM4_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM7_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - UART4_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - UART5_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USART1_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USART2_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USART3_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USBWakeUp_RMP_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USB_HP_CAN_TX_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USB_HP_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USB_LP_CAN_RX0_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - USB_LP_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - UsageFault_Handler from stm32f3xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f303xc.o(RESET)
  - WWDG_IRQHandler from startup_stm32f303xc.o(.text) referenced from startup_stm32f303xc.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f303xc.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f303xc.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  ADC4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  COMP1_2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  COMP4_5_6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  COMP7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  EXTI2_TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM1_BRK_TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM1_TRG_COM_TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM1_UP_TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USBWakeUp_RMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USB_HP_CAN_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USB_HP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  USB_LP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f303xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f303xc.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  EXTI0_IRQHandler (Thumb, 82 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.EXTI0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI0_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f303xc.o(RESET)

  HAL_Delay (Thumb, 32 bytes, Stack size 16 bytes, stm32f3xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> main

  HAL_GPIO_EXTI_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_hal_gpio.o(i.HAL_GPIO_EXTI_Callback))
  [Called By]

  - >> HAL_GPIO_EXTI_IRQHandler

  HAL_GPIO_EXTI_IRQHandler (Thumb, 18 bytes, Stack size 8 bytes, stm32f3xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_GPIO_EXTI_IRQHandler
  [Calls]
  - >> HAL_GPIO_EXTI_Callback
  [Called By]
  - >> EXTI0_IRQHandler

  HAL_GPIO_Init (Thumb, 364 bytes, Stack size 40 bytes, stm32f3xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> MX_GPIO_Init

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f3xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> main
  - >> MX_GPIO_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f3xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_Delay

  HAL_IncTick (Thumb, 12 bytes, Stack size 0 bytes, stm32f3xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f3xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 54 bytes, Stack size 16 bytes, stm32f3xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 122 bytes, Stack size 8 bytes, stm32f3xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f3xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> MX_GPIO_Init

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f3xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> HAL_MspInit
  - >> SystemClock_Config
  - >> MX_GPIO_Init

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f3xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_MspInit
  - >> HAL_Init

  HAL_RCC_ClockConfig (Thumb, 306 bytes, Stack size 32 bytes, stm32f3xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f3xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> SystemClock_Config

  HAL_RCC_GetSysClockFreq (Thumb, 84 bytes, Stack size 8 bytes, stm32f3xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 1424 bytes, Stack size 40 bytes, stm32f3xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f3xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f3xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f3xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f303xc.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f303xc.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(RESET)

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f3xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f303xc.o(RESET)

  SystemClock_Config (Thumb, 102 bytes, Stack size 72 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 136
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> main

  SystemInit (Thumb, 82 bytes, Stack size 0 bytes, system_stm32f3xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f303xc.o(.text)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f303xc.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 308 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 136
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_Init
  - >> HAL_GPIO_WritePin
  - >> HAL_Delay
  - >> SystemClock_Config
  - >> MX_GPIO_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  MX_GPIO_Init (Thumb, 128 bytes, Stack size 48 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f3xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  ### Undefined Global Symbols