Version 4
SymbolType CELL
RECTANGLE Normal -192 -368 192 320
TEXT 0 -8 Center 0 LT
WINDOW 0 0 -168 Center 0
WINDOW 3 0 152 Center 0
SYMATTR Value LT3598
SYMATTR Prefix X
SYMATTR SpiceModel LT3598.sub
SYMATTR Value2 LT3598
SYMATTR Description 6-String 30mA LED Driver with 1.5% Current Matching\n\nNote: Open LED logic and LED disable is not modeled.
PIN 192 -128 RIGHT 8
PINATTR PinName LED1
PINATTR SpiceOrder 1
PIN 192 -48 RIGHT 8
PINATTR PinName LED2
PINATTR SpiceOrder 2
PIN 192 32 RIGHT 8
PINATTR PinName LED3
PINATTR SpiceOrder 3
PIN 192 112 RIGHT 8
PINATTR PinName LED4
PINATTR SpiceOrder 4
PIN 192 192 RIGHT 8
PINATTR PinName LED5
PINATTR SpiceOrder 5
PIN 192 272 RIGHT 8
PINATTR PinName LED6
PINATTR SpiceOrder 6
PIN -192 192 LEFT 8
PINATTR PinName Iset
PINATTR SpiceOrder 8
PIN -192 32 LEFT 8
PINATTR PinName CTRL
PINATTR SpiceOrder 9
PIN -192 272 LEFT 8
PINATTR PinName Vc
PINATTR SpiceOrder 10
PIN 192 -208 RIGHT 8
PINATTR PinName FB
PINATTR SpiceOrder 11
PIN -192 112 LEFT 8
PINATTR PinName Tset
PINATTR SpiceOrder 12
PIN -192 -208 LEFT 8
PINATTR PinName PWM
PINATTR SpiceOrder 15
PIN -192 -128 LEFT 8
PINATTR PinName Rt
PINATTR SpiceOrder 16
PIN -64 320 BOTTOM 8
PINATTR PinName SS
PINATTR SpiceOrder 17
PIN -192 -48 LEFT 8
PINATTR PinName Vref
PINATTR SpiceOrder 18
PIN -192 -288 LEFT 8
PINATTR PinName _SHDN
PINATTR SpiceOrder 20
PIN -144 -368 TOP 8
PINATTR PinName Vin
PINATTR SpiceOrder 21
PIN 0 -368 TOP 8
PINATTR PinName SW
PINATTR SpiceOrder 22
PIN 144 -368 TOP 8
PINATTR PinName Vout
PINATTR SpiceOrder 23
PIN 192 -288 RIGHT 8
PINATTR PinName Vo_sw
PINATTR SpiceOrder 24
PIN 64 320 BOTTOM 8
PINATTR PinName GND
PINATTR SpiceOrder 25
