Version 4
SymbolType CELL
RECTANGLE Normal -256 -192 240 192
TEXT 0 0 Center 0 LT
WINDOW 0 0 -88 Center 0
WINDOW 3 0 56 Center 0
SYMATTR Value LTC3705
SYMATTR Prefix X
SYMATTR SpiceModel LTC3705.sub
SYMATTR Value2 LTC3705
SYMATTR Description Two-Switch Forward Controller and Gate Driver\n\nNote:  Fault Transmit and Receive are not modeled as is not slave mode.
PIN 0 192 BOTTOM 8
PINATTR PinName GND
PINATTR SpiceOrder 1
PIN 192 -192 TOP 8
PINATTR PinName IS
PINATTR SpiceOrder 2
PIN -144 192 BOTTOM 8
PINATTR PinName VSLMT
PINATTR SpiceOrder 3
PIN -256 -112 LEFT 8
PINATTR PinName UVLO
PINATTR SpiceOrder 4
PIN -256 112 LEFT 8
PINATTR PinName SSFLT
PINATTR SpiceOrder 5
PIN -208 -192 TOP 8
PINATTR PinName Ndrv
PINATTR SpiceOrder 6
PIN 240 -80 RIGHT 8
PINATTR PinName FB/IN+
PINATTR SpiceOrder 7
PIN 240 80 RIGHT 8
PINATTR PinName FS/IN-
PINATTR SpiceOrder 8
PIN 144 192 BOTTOM 8
PINATTR PinName PGND
PINATTR SpiceOrder 9
PIN 112 -192 TOP 8
PINATTR PinName BG
PINATTR SpiceOrder 10
PIN -256 0 LEFT 8
PINATTR PinName Vcc
PINATTR SpiceOrder 11
PIN -128 -192 TOP 8
PINATTR PinName Boost
PINATTR SpiceOrder 14
PIN -48 -192 TOP 8
PINATTR PinName TG
PINATTR SpiceOrder 15
PIN 32 -192 TOP 8
PINATTR PinName TS
PINATTR SpiceOrder 16
