Version 4
SymbolType CELL
RECTANGLE Normal -176 -224 176 224
TEXT 0 0 Center 0 LT
WINDOW 0 0 -103 Center 0
WINDOW 3 0 119 Center 0
SYMATTR Value LTC3418
SYMATTR Prefix X
SYMATTR SpiceModel LTC3418.sub
SYMATTR Value2 LTC3418
SYMATTR Description 8A, 4MHz, Monolithic Synchronous Step-down Regulator\n\nNote: Vref pin is not modeled and is assumed to be bypassed.  External Sync is also not modeled
PIN -176 176 LEFT 8
PINATTR PinName Rt
PINATTR SpiceOrder 1
PIN 176 176 RIGHT 8
PINATTR PinName Mode
PINATTR SpiceOrder 2
PIN -64 224 BOTTOM 8
PINATTR PinName SGND
PINATTR SpiceOrder 3
PIN 176 -48 RIGHT 8
PINATTR PinName SW
PINATTR SpiceOrder 4
PIN 64 224 BOTTOM 8
PINATTR PinName PGND
PINATTR SpiceOrder 5
PIN 64 -224 TOP 8
PINATTR PinName PVin
PINATTR SpiceOrder 6
PIN -64 -224 TOP 8
PINATTR PinName SVin
PINATTR SpiceOrder 7
PIN 176 -160 RIGHT 8
PINATTR PinName Pgood
PINATTR SpiceOrder 8
PIN 176 64 RIGHT 8
PINATTR PinName FB
PINATTR SpiceOrder 9
PIN -176 64 LEFT 8
PINATTR PinName Ith
PINATTR SpiceOrder 10
PIN -176 -48 LEFT 8
PINATTR PinName Run/SS
PINATTR SpiceOrder 11
PIN -176 -160 LEFT 8
PINATTR PinName Track
PINATTR SpiceOrder 12
