Version 4
SymbolType CELL
RECTANGLE Normal -400 -544 400 544
TEXT 0 0 Center 2 LT
WINDOW 0 0 -240 Center 2
WINDOW 3 0 240 Center 2
SYMATTR Value LTC3861
SYMATTR Prefix X
SYMATTR SpiceModel LTC3861.sub
SYMATTR Value2 LTC3861
SYMATTR Description Dual, Multiphase Step-Down Voltage Mode DC/DC Controller with Accurate Current Sharing\n\nNote:  Internal soft-start timer is reduced to 0.5ms from 2ms
PIN -400 0 LEFT 8
PINATTR PinName FB1
PINATTR SpiceOrder 1
PIN -400 -96 LEFT 8
PINATTR PinName COMP1
PINATTR SpiceOrder 2
PIN -400 192 LEFT 8
PINATTR PinName Vsnsp1
PINATTR SpiceOrder 3
PIN -400 288 LEFT 8
PINATTR PinName VsnsN1
PINATTR SpiceOrder 4
PIN -400 96 LEFT 8
PINATTR PinName Vsnsout1
PINATTR SpiceOrder 5
PIN 400 96 RIGHT 8
PINATTR PinName Vsnsout2
PINATTR SpiceOrder 6
PIN 400 288 RIGHT 8
PINATTR PinName VsnsN2
PINATTR SpiceOrder 7
PIN 400 192 RIGHT 8
PINATTR PinName Vsnsp2
PINATTR SpiceOrder 8
PIN 400 -96 RIGHT 8
PINATTR PinName COMP2
PINATTR SpiceOrder 9
PIN 400 0 RIGHT 8
PINATTR PinName FB2
PINATTR SpiceOrder 10
PIN 400 384 RIGHT 8
PINATTR PinName TK/SS2
PINATTR SpiceOrder 11
PIN -144 544 BOTTOM 8
PINATTR PinName Freq
PINATTR SpiceOrder 12
PIN -400 480 LEFT 8
PINATTR PinName CLKIN
PINATTR SpiceOrder 13
PIN 400 480 RIGHT 8
PINATTR PinName Clkout
PINATTR SpiceOrder 14
PIN -48 544 BOTTOM 8
PINATTR PinName PhaseMD
PINATTR SpiceOrder 15
PIN 192 -544 TOP 8
PINATTR PinName Pgood2
PINATTR SpiceOrder 16
PIN 400 -480 RIGHT 8
PINATTR PinName PWMEN2
PINATTR SpiceOrder 17
PIN 400 -384 RIGHT 8
PINATTR PinName PWM2
PINATTR SpiceOrder 18
PIN 288 -544 TOP 8
PINATTR PinName Run2
PINATTR SpiceOrder 19
PIN 240 544 BOTTOM 8
PINATTR PinName Ilim2
PINATTR SpiceOrder 20
PIN 48 544 BOTTOM 8
PINATTR PinName SGND
PINATTR SpiceOrder 21
PIN 400 -288 RIGHT 8
PINATTR PinName Sense2p
PINATTR SpiceOrder 22
PIN 400 -192 RIGHT 8
PINATTR PinName Sense2n
PINATTR SpiceOrder 23
PIN -400 -192 LEFT 8
PINATTR PinName Sense1n
PINATTR SpiceOrder 24
PIN -400 -288 LEFT 8
PINATTR PinName Sense1p
PINATTR SpiceOrder 25
PIN -240 544 BOTTOM 8
PINATTR PinName Ilim1
PINATTR SpiceOrder 27
PIN -288 -544 TOP 8
PINATTR PinName Run1
PINATTR SpiceOrder 28
PIN -400 -384 LEFT 8
PINATTR PinName PWM1
PINATTR SpiceOrder 29
PIN -400 -480 LEFT 8
PINATTR PinName PWMEN1
PINATTR SpiceOrder 30
PIN -192 -544 TOP 8
PINATTR PinName Pgood1
PINATTR SpiceOrder 31
PIN 144 544 BOTTOM 8
PINATTR PinName Iavg
PINATTR SpiceOrder 32
PIN 96 -544 TOP 8
PINATTR PinName CONFIG
PINATTR SpiceOrder 33
PIN -96 -544 TOP 8
PINATTR PinName Vinsns
PINATTR SpiceOrder 34
PIN -400 384 LEFT 8
PINATTR PinName TK/SS1
PINATTR SpiceOrder 35
PIN 0 -544 TOP 8
PINATTR PinName Vcc
PINATTR SpiceOrder 36
