Version 4
SymbolType CELL
RECTANGLE Normal -352 -192 352 192
TEXT 0 0 Center 0 LT
WINDOW 0 0 -64 Center 0
WINDOW 3 0 64 Center 0
SYMATTR Value LTC3706
SYMATTR Prefix X
SYMATTR SpiceModel LTC3706.sub
SYMATTR Value2 LTC3706
SYMATTR Description Secondary-Side Synchronous Forward Controller with PolyPhase Capability NOTE:  Fault Transmit, Fault Receive, PolyPhase Capability, and the differential amplifier are not modeled.
PIN -96 -192 TOP 8
PINATTR PinName SG
PINATTR SpiceOrder 1
PIN -288 -192 TOP 8
PINATTR PinName FG
PINATTR SpiceOrder 2
PIN 288 -192 TOP 8
PINATTR PinName Pgood
PINATTR SpiceOrder 3
PIN 192 192 BOTTOM 8
PINATTR PinName Mode
PINATTR SpiceOrder 4
PIN 352 64 RIGHT 8
PINATTR PinName FB
PINATTR SpiceOrder 6
PIN 352 128 RIGHT 8
PINATTR PinName Ith
PINATTR SpiceOrder 7
PIN -352 128 LEFT 8
PINATTR PinName Run/SS
PINATTR SpiceOrder 8
PIN -288 192 BOTTOM 8
PINATTR PinName GND
PINATTR SpiceOrder 12
PIN 288 192 BOTTOM 8
PINATTR PinName FS/Sync
PINATTR SpiceOrder 13
PIN 96 192 BOTTOM 8
PINATTR PinName SLP
PINATTR SpiceOrder 14
PIN -352 -128 LEFT 8
PINATTR PinName Is-
PINATTR SpiceOrder 15
PIN -352 -64 LEFT 8
PINATTR PinName Is+
PINATTR SpiceOrder 16
PIN 0 192 BOTTOM 8
PINATTR PinName RegSD
PINATTR SpiceOrder 17
PIN 96 -192 TOP 8
PINATTR PinName NDRV
PINATTR SpiceOrder 18
PIN 0 -192 TOP 8
PINATTR PinName Vin
PINATTR SpiceOrder 19
PIN -192 -192 TOP 8
PINATTR PinName SW
PINATTR SpiceOrder 20
PIN -352 64 LEFT 8
PINATTR PinName PT-
PINATTR SpiceOrder 21
PIN -352 0 LEFT 8
PINATTR PinName PT+
PINATTR SpiceOrder 22
PIN -192 192 BOTTOM 8
PINATTR PinName PGND
PINATTR SpiceOrder 23
PIN 192 -192 TOP 8
PINATTR PinName Vcc
PINATTR SpiceOrder 24
PIN 352 0 RIGHT 8
PINATTR PinName Vsout
PINATTR SpiceOrder 9
PIN 352 -64 RIGHT 8
PINATTR PinName Vs-
PINATTR SpiceOrder 11
PIN 352 -128 RIGHT 8
PINATTR PinName Vs+
PINATTR SpiceOrder 10
PIN -96 192 BOTTOM 8
PINATTR PinName Phase
PINATTR SpiceOrder 5
