Version 4
SymbolType CELL
RECTANGLE Normal -272 -176 272 176
TEXT 0 0 Center 0 LT
WINDOW 0 0 -64 Center 0
WINDOW 3 0 64 Center 0
SYMATTR Value LTC3726
SYMATTR Prefix X
SYMATTR SpiceModel LTC3726.sub
SYMATTR Value2 LTC3726
SYMATTR Description Secondary-Side Synchronous Forward Controller\n\nNote:  Fault Transmit, Fault Receive, PolyPhase Capability, and the differential amplifier are not modeled.
PIN 64 -176 TOP 8
PINATTR PinName SG
PINATTR SpiceOrder 1
PIN -192 -176 TOP 8
PINATTR PinName FG
PINATTR SpiceOrder 2
PIN 192 176 BOTTOM 8
PINATTR PinName Mode
PINATTR SpiceOrder 3
PIN 272 -32 RIGHT 8
PINATTR PinName FB
PINATTR SpiceOrder 4
PIN 272 32 RIGHT 8
PINATTR PinName Ith
PINATTR SpiceOrder 5
PIN 272 96 RIGHT 8
PINATTR PinName Run/SS
PINATTR SpiceOrder 6
PIN 64 176 BOTTOM 8
PINATTR PinName SLP
PINATTR SpiceOrder 7
PIN -192 176 BOTTOM 8
PINATTR PinName GND
PINATTR SpiceOrder 8
PIN 272 -96 RIGHT 8
PINATTR PinName FS/Sync
PINATTR SpiceOrder 9
PIN -272 -96 LEFT 8
PINATTR PinName Is-
PINATTR SpiceOrder 10
PIN -272 -32 LEFT 8
PINATTR PinName Is+
PINATTR SpiceOrder 11
PIN -64 -176 TOP 8
PINATTR PinName SW
PINATTR SpiceOrder 12
PIN -64 176 BOTTOM 8
PINATTR PinName PGND
PINATTR SpiceOrder 13
PIN -272 96 LEFT 8
PINATTR PinName PT-
PINATTR SpiceOrder 14
PIN -272 32 LEFT 8
PINATTR PinName PT+
PINATTR SpiceOrder 15
PIN 192 -176 TOP 8
PINATTR PinName Vcc
PINATTR SpiceOrder 16
