Version 4
SymbolType CELL
RECTANGLE Normal -144 -128 144 144
TEXT 0 0 Center 0 LT
WINDOW 0 0 -80 Center 0
WINDOW 3 0 80 Center 0
SYMATTR Value LTC3529
SYMATTR Prefix X
SYMATTR SpiceModel LTC3529.sub
SYMATTR Value2 LTC3529
SYMATTR Description 1.5A, 1.5MHz Step-up DC/DC Converter in 2mm×3mm DFN\n\nNote: 1/4th of the real internal soft-start time is presented, on purpose of saving simulation time.
PIN 144 -48 RIGHT 8
PINATTR PinName Vout
PINATTR SpiceOrder 1
PIN 64 -128 TOP 8
PINATTR PinName SW
PINATTR SpiceOrder 2
PIN -144 64 LEFT 8
PINATTR PinName _SHDN
PINATTR SpiceOrder 3
PIN 64 144 BOTTOM 8
PINATTR PinName PGND
PINATTR SpiceOrder 4
PIN -144 -48 LEFT 8
PINATTR PinName _Fault
PINATTR SpiceOrder 5
PIN -64 144 BOTTOM 8
PINATTR PinName SNSGND
PINATTR SpiceOrder 6
PIN 144 64 RIGHT 8
PINATTR PinName RST
PINATTR SpiceOrder 7
PIN -64 -128 TOP 8
PINATTR PinName Vin
PINATTR SpiceOrder 8
